AUTO INHIBITOR SWITCH  WIRING

[image: A diagram of a car light

AI-generated content may be incorrect.]WHERE DOES THESE TWO WIRES GO



The reversing circuit I understand, and my lights work.

My auto conversation will not start until I am in P or N which is correct.

I need to see where the wires were connected to by my mechanic so really I just doing my research while I am away from home at work.

For sure my ROVERGAUGE tells me I am still manual and the vehicle drives and runs, but I think it’s in some sort of limp mode as the fuel usage is higher than when it was a manual gearbox.

No fault codes on the rovergauge program

1) The wires BY and BO should one of these go to pin 34 on the 14CUX?
2) Previously had a manual box a lot of info about a 510 ohm resistor to ground? Where is the resistor?
3) So if I check the ECU and pin 34 is connected to ground then I simply disconnect it and reroute the wire from pin 34 via the in inhibitor switch on the side of my gearbox?  

Many thanks in advance for any advice…………………cheers Ivan 
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